|  |  |  |
| --- | --- | --- |
| Description | Quantity | UOM |
| ACB, PN: Masterpact NW25H1, 2500A, 4 Poles, Icu= 65KA, Uimp= 12 KV, Withdrawable CB, With micrologic 6.0E LSIG Trip Unit, Includes (UC1, UC2, UC3, MCH, XF, MN, SDE1, OF1, OF2, OF3, OF4),  | 1 | Each |
| ACB, PN: M-Pact MPA31W10, 1000A, 3 Poles, Icu= 50KA, Withdrawable CB, With Digital Trip Unit, Includes (Shunt Release ST, Closing Release CC, Spring Charging Motor),  | 1 | Each |
| ACB, PN: Masterpact NT10H1, 1000A, 3 Poles, Icu= 42KA, Uimp= 12 KV, Withdrawable CB, With micrologic 6.0E LSIG Trip Unit, Includes (UC1, UC2, UC3, MCH, XF, MN, SDE1, OF1, OF2, OF3, OF4), SCHNEIDER ELECTRIC | 1 | Each |
| Automatic Transfer Switch Controller, PN: ATyS C30, With RJ45 terminal,  | 2 | Each |
| Remote Control Interface, PN: ATyS D20, With RJ45 terminal,  | 2 | Each |
| Multi-function Timer, PN: RE17RMMU, 1 C/O, T= (0.1s - 100h), Supply Voltage = (24 - 240 VAC) / (24 VDC), Nominal Output = 8A/250V,  | 2 | Each |
| Under/Over Voltage Relay, PN: RM35TF30, Uc = (220-480V), Measurment Range = (220 - 480V), Nominal Output = 5A / 250V,  | 2 | Each |
| Power Supply, PN: M-PRO APU PLC, Input: (175 - 275 VDC, 175 - 275 VAC 50Hz), Output:( 22 - 26 VDC), Output Power ? 9.6 W,  | 2 | Each |
| High-Capacity Dual Position Relay, PN: DCS-11, 220 VDC, Shanghai Relay Co. | 2 | Each |
| Relay, PN: JZX54P, 220 VDC, 14 Pins,  | 2 | Each |
| Engine Generator Controller, PN: DSE 7310 MKII 7310-010-03, DC Supply: 8-35 V 0.5 A Max, DC Outputs: 24 V / 15 A (4-5) 2 A (8-13), DC Inputs: 30 V , Comms Port: 5 V Max, | 1 | Each |
| Automatic Battery Charger, PN: SNTL150P, Input Voltage = (95 - 265 ) VAC, Input Frequency = (47 - 63) Hz, Max. Input Current = 3 A, DC Output = 24 VDC / 5 A, Float Voltage = 27.6 VDC, Boost Voltage = 31.2 VDC,  | 1 | Each |
| Definite Purpose Contactor, PN: 45FG20AG, 2 Poles, Full Load Current (FLA) = 35 A, Coil: (190 - 220 VAC) / 50 Hz) or (208 - 240 VAC) / 60 Hz, Open Enclosure,  | 2 | Each |
| Battery Charger, P.N : D-292865 ,AC input 120/240VAC, 50/60Hz,1 Phase , 5.1/3A, DC output 26VDC, 10A, Allowable range of battery capacities : 50-200 AH ;  | 1 | Each |